ST-102M

    Application:   Dual angle for near or far-field floor

                               monitoring. Stand mount  for main side fill. 

    Loudspeaker Type: Two-way bass reflex 

    LF Driver:  10" 

    HF Unit:  Compression driver on constant directivity horn 

    Protection Circuitry:  Yes 

    Frequency Response:  80Hz to 16,000 Hz 

    Long Term Power Handling Capacity:   75 watts 

    Nominal Impedance:  8 ohms 

    Sensitivity, 1 Watt @ 1 Meter:    98 dB 

    Crossover Frequency:  3 kHz (12dB/octave) 

    Nominal Dispersion:  40degree H x 90degree V 

    Attenuation Circuitry:  No 

    Connectors:  Two 1/4" 

    Standmount:  Yes 

    Dimensions:  H - 12.63" W - 19.38" D - 12.5" 

    Weight:  23 lbs

